*) Rack Mount System

1. 개요

본 기기는 네트워크 분배기로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Allows for 2 XLR analog inputs, each splayed to three parallel outputs

Accepts OpticalCON and EtherCON connections

Combines Primary & Secondary LAN to a single cable, carrying redundant networked audio to the loudspeaker system

Requires two external AVB Milan enabled switches for redundant operation

3. 규격 및 사양

Connection	: 2x XLR in, 6x XLR out, 26x etherCON, 8x	opticalCON

Height Front (mm / in)	: 88 / 3.46

Width (mm / in)	: 483 / 19

Depth (mm / in)	: 257 / 10.1

* CS Network Distribution System(NDS) 동급이상품