*) Rack Mount System

1. 개요

본 기기는 전원 분배기로 다음과 같은 규격에 준한다.

2. 기능 및 특성

6 circuits of 208/220v, 16A power

CEE 3-phase (230V regions) and L21-30 (110V regions)

Data port to connect to AI software providing power consumption monitoring

Additional EMI/EMC filtration to improve noise rejection

Power outputs are offered through 6x powerCON and 1x Socapex on the front panel

Front LED status lights

Contains 2 x powerCON aux outlets on the rear, tied to a 5A Aux breaker

3. 규격 및 사양

Connection	: 8x powerCON True1 out (6x Spk. Out, 2x Aux	Out), 1x Socapex 19 Out, 1x 32A CEE In (230V	Version), 2x L21-30 In (110V Version), 1x	etherCON

Height Front (mm / in)	: 88 / 3.46

Width (mm / in)	: 483 / 19

Depth (mm / in)	: 488 / 19.2

* CS Power Dditribution System(PDS) 동급이상품