*) 2-WAY POWERED LINE ARRAY SYSTEM

1. 개요

본 기기는 2-Way 앰프 내장형 라인어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

MILAN 네트워크 AV 시스템

여러가지 소스를 데이지 체인 방식으로 연결

소프트웨어를 통한 모니터링

2x ND10-LM 10” Kevlar Neodymium Driver

Adamson NH4 4” Diaphragm / 1.5” Exit Compression Driver

80° x 10°(H x V) 지향각

해양 등급 자작나무 합판 및 항공기 등급의 강철과 알루미늄으로 제작된 캐비닛

SlideLock 연결 시스템

3. 규격 및 사양

Frequency Range (+/- 3dB)	: 60 Hz - 18 kHz

Nominal Directivity (-6 dB) H x V	: 80° x 10°

Maximum Peak SPL	: 141.3 dB

Components LF	: 2x ND10-LM 10” Kevlar Neodymium Driver

Components HF	: Adamson NH4 4” Diaphragm / 1.5” Exit	Compression Driver

Rigging	: Slidelock Rigging System

Connections

Power	: powerCON TRUE1

Network	: 2 x etherCON

Analog	: 2 x XLR

Height Front (mm / in)	: 265 / 10.4

Height Back (mm / in)	: 178 / 7

Width (mm / in)	: 737 / 29

Depth (mm / in)	: 526 / 20.7

Weight (kg / lbs)	: 31 / 68.4

Amplification	: 2 channel Class-D, 2400 W total output

Input Voltage	: 100 - 240 V

Current Draw at 230 V	: 0.45 A rms idle, 1.6 A rms long-term, 10 A	max peak

Processing	: Onboard / Proprietary

* CS10n 동급이상품