*) SUBWOOFER

1. 개요

본 기기는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2x ND15-S 15” Kevlar Neodymium Driver

Built-in M20 Thread, 5/16-18 Threads for Eye-hooks

3. 규격 및 사양

Frequency Range (+/- 3dB)	: 40Hz - 160Hz

Maximum Peak SPL	: 136.3 dB

Components LF	: 2x ND15-S 15” Kevlar Neodymium Driver

Nominal Impedance LF	: 4 Ω

Power Handling (AES / Peak) LF	: 2x 500 / 2x 2000 W

Rigging	: Built-in M20 Thread, 5/16-18 Threads for	Eye-hooks

Connection	: 2x Speakon™ NL4 (Barrier Strip Optional)

Height Front (mm / in)	: 619 / 24.38

Width (mm / in)	: 540 / 21.25

Depth (mm / in)	: 757 / 29.88

Weight (kg / lbs)	: 47 / 103.5

Processing	: Lake, XTA

* POINT 215SUB 동급이상품