*) 3-WAY LINE ARRAY SYSTEM

1. 개요

본 기기는 3-Way 라인어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Including 8 transducers, amplification, a networked DSP endpoint, Autolock rigging into a lightweight

M140 MF compression drivers introduce  and the 3” HF compression drivers

90° x 6°(H x V) 지향각

해양 등급 자작나무 합판 및 항공기 등급의 강철과 알루미늄으로 제작된 캐비닛

Integrated Rigging System

3. 규격 및 사양

Frequency Range (+/- 3dB)	: 50 Hz - 20 kHz

Nominal Directivity (-6 dB)	: H x V 90° x 6°

Maximum Peak SPL	: 151 dB

LF Component	: 2x ND13-S 13” Kevlar Neodymium Driver

Directional Component	: 2x ND10-LM 10” Kevlar Neodymium Driver

MF Component	: 2x M140 Kevlar Compression Driver

HF Component	: 2x 3” Compression Driver

Rigging	: Autolock™ Rigging

Connection	: 2x etherCON™ - passive continuity when	powerless, Analog : XLR3 in & thru, powerCON	TRUE1 TOP in & thru

Height Front (mm / in)	: 338 / 13.3

Height Back (mm / in)	: 286 / 11.25

Width (mm / in)	: 1306 / 51.4

Depth (mm / in)	: 562 / 22.1

Weight (kg / lbs)	: 85 / 188

Colour	: Black & White (Standard), RAL Colours (On	Demand)

Amplification	: 5 channel Onboard Class-D, SMPS

Processing	: Onboard, controllable through proprietary	software

* VGt 동급이상품