*) TWO-WAY PASSIVE SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2-way design - 6.5” woofer and 1” tweeter

70V/100V/8Ω operation

Power handling: 50W (RMS), 100W (PMPO)

Transformer taps at 100V (20W, 40W, 8Ω) and 70V (10W, 20W, 40W, 8Ω)

Weather-resistant design for exterior use

Paintable white cabinet and grille

Adjustable angle wall-mount bracket included

3. 규격 및 사양

Low-Frequency Driver	: 6.50" (165.5mm)

High-Frequency Driver	: 1" (25mm)

Power	: 50W RMS

Impedance	: 8Ω

Transformer Taps	: 70V, 100V

Frequency Response	: 60 Hz - 20 kHz

Sensitivity	: 86 dB ± 2 dB (1W/1m)

Dimensions (WxHxD)	: 138 x 296 x 181 mm

Weight	: 4.16kg

* DN-205IO 동급이상품