*) MEDIA PLAYER

1. 개요

본 기기는 CD, USB, 블루투스 등을 연결하여 사용 할 수 있는 재생 및 녹음 플레이어로 AM/FM 튜너 기능을 가지고 있으며 다음과 같은 규격에 준한다.

2. 기능 및 특성

Super-fast loading, slot-in CD mechanism

Supports removable USB thumb and HDDs, SD/SDHC cards

Wireless audio playback from devices via BluetoothTM

Plays CD, MP3, WAV, and AAC files

3.5mm Aux-in for audio playback of other devices

AM/FM Tuner w/ dedicated audio out for multi-room use

Unbalanced combi audio output

10-key direct track access

Random, Repeat One, Repeat All, and continuous play modes

Folder only and All play modes

IR controllable with included, compact remote

1RU chassis with removable rack ears

Detachable IEC-weighted AC inlet

100-220v switching power supply

3. 규격 및 사양

System	: CD/Media Player with Bluetooth Receiver and	Tuner

Compatible media	: CD, USB device (mass storage class),	SD/SDHC

Playable formats, file systems

- CD	: CD-DA (CD-TEXT), CD-ROM (ISO9660), CD-R,	MP3-CD

- USB	: FAT16 / FAT32

- SD/SDHC	: FAT16 / FAT32

Number of channels	: 2 (stereo), 1 (mono)

Audio frequency characteristics	: 10Hz – 20kHz (+ 1.0 dB)

S/N ratio	: More than 95 dB (A-Weighted)

Total harmonic distortion	: Less than 0.01%

Dynamic range	: More than 85 dB

Channel separation	: More than 80 dB

Bluetooth Version	: 3.0

Tuner Section

- Usable sensitivity	: FM: 30 dBμV / m

: AM: 60 dBμV / m

- Channel separation	: 20 dB (0 kHz)

- S/N ratio	: FM: More than 40 dB

: AM: More than 30 dB

- THD+N (1 kHz)	: Monoaural 3.0%, Stereo 3.0%

Analog Out L/R

– Type	: RCA terminal

– Load impedance	: Over 10 kΩ/kohms

– Output level	: 2 Vrms / at 10 kΩ/kohms load

AUX–In

– Type	: TRS terminal (Ø 3.5)

– Input impedance	: Over 10kΩ/kohms

– Maximum input level	: 1 Vrms

– Maximum output level	: 3 Vrms

Power consumption	: 30W

Dimensions (HxWxD)	: 44.5 x 482.6 x 347 mm

* DN-300Z 동급이상품