*) MEDIA PLAYER

1. 개요

본 기기는 CD, USB, 블루투스 등을 연결하여 음원 소스를 재생하는 플레이어로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Bluetooth 5.0 pairing to (8) devices

Slot-loading CD transport

USB host port for file playback

10-button direct track access

3.5mm AUX input for playback from portable players

RS-232c control capable

Compact IR remote control included

Balanced (XLR) and unbalanced (RCA) outputs

3. 규격 및 사양

Audio channels	: 2 channels / stereo

Frequency response	: 10 - 20,000 Hz, +/- 1.0dB

Dynamic range	: > 85dB (10- 20,000 Hz A-weighted)

Signal to Noise ratio	: > 90dB (1kHz, 0db, A-weighted)

Channel separation	: > 80dB (1kHz, 0dB, A-weighted)

Total Harmonic Distortion (THD)	: < 0.01% (1kHz, 0dB, A-weighted)

Bluetooth version	: 5.0

Outputs

- XLR (balanced)	: 2.0Vrms

- RCA (unbalanced)	: +4dBu

Remote Control

- IR Remote	: Infrared protocol / NEC format

: Transmit output level : >200mVp-p

Serial Remote

- D-sub 9-pin female RS-232C

- Mode	: Full duplex

- Baud rate	: 9600/38400 b/s (selectable in the menu)

- Data	: 8bits

- Start bit	: 1bit

- Stop bit	: 1bit

Audio File / SIGNAL

- Sample rate	: CD-DA, Audio file 44.1kHz

- Word length	: CD-DA, Audio file 16-bit

- File format	: Audio file WAV/MP3/AAC

- Bit rate	: MP3, AAC, CBR/VBR ST/Mono 32~320kps

- ID3 tag	: MP3 V1.x~2.4

CD Drive

- Media	: File system: CD-DA (CD-TEXT), CD-ROM	(ISO9660)

: Disc: CD, CD-R

USB Storage Device

- File system	: FAT 16/32

- Media type	: Flash/ HDD

Power requirements	: 100-230 VAC

Power consumption	: <30W

LCD Display	: LCD 2 lines, 16 characters x 2 lines LCM	display

Dimensions	: 483 x 347 x 44 mm

Weight	: 2.92kg

* DN-500CB 동급이상품