*) MEDIA PLAYER

1. 개요

본 기기는 CD, USB, 블루투스 등을 연결하여 음원 소스를 재생하는 플레이어로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Plays content from SD/SDHC, USB/HDD, 3.5mm and Bluetooth

Mic/Line XLR front panel combo jack input with gain control and 48VDC phantom power

Pair up to (8) Bluetooth devices for playback

Balanced XLR and unbalanced RCA outputs

Control via front panel or included IR remote

Pitch and tempo control +/- 15%

3. 규격 및 사양

Frequency Response	: 20 Hz – 20 kHz (+/- 1.0dB)	20 Hz – 20 kHz (+/- 1.0dB)

Dynamic Range	: > 85 dB

Signal-to-Noise Ratio	: > 90 dB (A-weighted0

Variable Pitch/Tempo Control	: ±15%

Audio File Formats Supported

- WAV (44.1k, 16bit)

- MP3 (44.1k, from 64 to 320 kbit/s)

- MP2

- M4A (without DRM protection)

- WMA (without DRM protection)

Bluetooth Version	: v4.0 / v2.1 + EDR

Connectors

- (2) Balanced XLR outputs

- (1) Unbalanced RCA stereo output pair

- (1) Balanced XLR-1/4 input

- (1) 1/8” Aux (3.5 mm) input

- (2) USB ports

- (1) 1/4" Headphone output

- (1) IEC power input

Input Voltage	: 100–240 V, 50/60 Hz

Fuse	: 1A

Consumption	: 21W

Dimensions (WxDxH)	: 430 x 200 x 43.6 mm

Weight	: 2.3kg

* DN-F350 동급이상품