*) Omni Miniature Lavalier Microphone

1. 개요

본 기기는 바운더리 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Exceptional audio quality

Uniform, consistent sound between DPA mics

Extremely rugged and reliable

Diminutive size made for flexible and easy concealment

Large selection of clips, windscreens, grids and other accessories

Modular adapter system fits most professional wireless systems

3. 규격 및 사양

Directional pattern	: Omnidirectional

Principle of operation	: Pressure

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range ±2 dB	: Soft boost grid: 20 Hz - 20 kHz, 3 dB soft	boost at 8 - 20 kHz. High boost grid: 20 Hz -	20 kHz, 10 dB boost at 12 kHz

Sensitivity, nominal, ±3 dB at 1 kHz	: 20 mV/Pa; -34 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 23 dB(A) re. 20 µPa (max. 26 dB(A))

Equivalent noise level, ITU-R BS.468-4	: Typ. 35 dB (max. 38 dB)

Distortion, THD < 0.5%	: 128 dB SPL RMS, 131 dB SPL peak

Distortion, THD < 1%	: 129 dB SPL RMS, 132 dB SPL peak

Dynamic range	: Typ. 106 dB

Max. SPL, THD 10%	: 134 dB SPL peak

Rated output impedance	: 30 - 40 Ω

Cable drive capability	: Up to 300 m (984 ft) with DAD6001-BC XLR	Adapter

Power supply (for full performance)	: For wireless systems Min. 5 V - max. 10 V	through DPA adapter With DAD6001-BC: P48	(Phantom Power). Will work from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD6001-BC XLR Adapter

Connector	: MicroLock

Weight	: 7.5 g incl. Cable and MicroLock connector

Microphone diameter	: 5.4 mm

Microphone length	: 12.7 mm

Cable length	: 3 m

* 4060-OP-C-B90-3 동급이상품