*) AES50 REPEATER

1. 개요

본 기기는 장거리 디지털 신호를 전송할 때 감쇠하는 신호를 새롭게 재생하여 다시 전달하는 재생 중계 장치로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Extends two independent AES50 connections by up to 100 m with CAT5 cable

High channel capacity - 48 channels @ 96 kHz or 96 channels @ 48 kHz bidirectional operation

Supports dual-redundant AES50 networks (X and Y connections)

Rugged locking Neutrik etherCON connectors used for AES50 connections

Status indicator LEDs on front panel for each AES50 port

Dual-redundant power supply inputs with locking Switchcraft* connectors

External auto-ranging universal switch-mode power supply adapter

Aluminium extrusion casing with stackable protective silicone rubber sleeve

3. 규격 및 사양

AES50

- Ports	: 2 Input, 2 Output

- Type	: Neutrik etherCON

- Sample Rate	: 48 kHz, 96 kHz

Other Terminations

- Power	: 2

- Type	: Switchcraft locking 2.1 mm DC power	connector (centre positive)

Power Requirements

- Voltage	: +9 V to +18 V DC

- Consumption	: 83 mA (single channel),	166 mA (both channels)

Dimensions (WxDxH)	: 106 x 145 x 59 mm

Weight	: 0.8 kg

* DN9610 동급이상품