*) CONVERTER

1. 개요

본 기기는 AES50 신호를 USB로 전환하여 주는 컨버터로 다음과 같은 규격에 준한다.

2. 기능 및 특성

AES50 to USB 2.0 converter for simultaneous computer audio recording and playback

Up to 48 bidirectional channels @ 48 kHz and 24 bidirectional channels @ 96 kHz

Switchable 48 kHz and 96 kHz sample rate operation

Operates from incoming AES50 clock

Powered via USB 2.0 interface

Native Core Audio driver support in Mac OS X, software drivers available for Windows PC

LED indicators monitor network activity and speed

Compact and rugged design with durable aluminium extrusion casing

3. 규격 및 사양

Sample rates	: 48 kHz, 96 kHz

Bit depth (Resolution)	: 24-Bit

AES50 Audio channels (48 kHz)	: Up to 48 bidirectional channels

AES50 Audio channels (96 kHz)	: Up to 24 bidirectional channels

Clock source	: Incoming AES50 clock

AES50 Interface Connector type	: Neutrik etherCON with LED status indicators

USB Interface Connector type	: USB 2.0 Type B

Ethernet Control Port Connector type : RJ-45

Dimensions (WxDxH)	: 119 x 150 x 64 mm

Weight	: 0.5 kg

* DN9630 동급이상품