*) NETWORK BRIDGE

1. 개요

본 기기는 디지털 콘솔과 디지털 I/O 하드웨어, 오디오 레코더 및 기타 AES50 장비에 다양한 멀티채널 오디오 네트워크 연결이 가능한 네트워크 브릿지로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Network bridge format converter for AES50 networks with up to 64 bidirectional channels

Compatible with AES50, DANTE, MADI and USB network modules

Asynchronous sample rate conversion on every channel with bypass facility

Bidirectional output audio clock inhibit feature for redundant network systems

24 bit audio operation with 96 kHz and 48 kHz sample rates

Video synchronisation in standard and high defi nition formats

Internal “AES Grade 1” temperaturecompensated word clock (1 ppm)

Internal web server allows browserbased confi guration via Ethernet control port

Status indicator LEDs and LCD display on front panel

Features Neutrik etherCON* network ports

Rugged 1U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

AES50 Ports	: 3

- Type	: Neutrik etherCON with LED status indication

- Sample rate	: 48 kHz, 96 kHz

Ethernet Control Port	: 1

- Type	: Neutrik etherCON with LED status indication

Word clock input	: 1

- Type	: Neutrik BNC with 75 ohm termination

- Sample rate	: 48 kHz, 96 kHz

Word clock output	: 1

- Type	: Neutrik BNC (no termination)

- Sample rate	: 48 kHz, 96 kHz

Video black burst input	: 1

- Type	: Neutrik BNC with 75 ohm termination

- Formats	: Standard defi nition: PAL, SECAM, NTSC

: High defi nition: 720P, 1080P, 1080i

Network Module Expansion Slot	: 1

Power Requirements

- Voltage	: 100 to 240 VAC, 50 to 60 Hz

- Consumption	: <50W

Dimensions (WxDxH)	: 483 x 411 x 44 mm

Weight	: 5.1 kg

* DN9650 동급이상품