*) AES50 EXTENDER

1. 개요

본 기기는 여러 선로의 네트워크 오디오 신호를 하나의 선로로 통합하여 분배/전송 가능한 익스텐더로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Multiplexes up to 8 AES50 connections into one optical fibre cable or CAT5 cable

Extends AES50 connections up to 1,000 m with optical fibre or 100 m with CAT5 cable

High channel capacity with 192 bidirectional channels @ 96 kHz

Internal “AES Grade 1” temperaturecompensated  word clock (1 ppm)

Neutrik etherCON* connectors used for AES50 ports and copper snake connection

Dual-fibre Neutrik opticalCON DUO connector used for optical fibre snake connection

Internal web server allows browser-based configuration via Ethernet control port

Rugged 1U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

AES50 Ports

- Type	: Neutrik etherCON with LED status indication

- Sample rate	: 96 kHz or 48 kHz

Ethernet Control Port

- Type	: Neutrik etherCON with LED status indication

Copper Snake Port

- Type	: Neutrik etherCON

Optical Snake Port

- Type	: Neutrik opticalCON DUO

- Optical fibre	: Single-mode or Multi-mode dual fibre

Onboard Clock

- Type	: Temperature-controlled crystal oscillator (TCXO)	with 1 part-per-million (1 ppm) stability

Clock Source

- Options	: Internal clock, External AES50 clock,	External snake clock

Power Requirements

- Voltage	: 100 to 240 VAC, 50 to 60 Hz

- Consumption	: <50 W

Dimensions (WxDxH)	: 483 x 412 x 44 mm

Weight	: 5.1 kg

* DN9680 동급이상품