*) NETWORK MODULE

1. 개요

본 기기는 DANTE 신호를 연결하기 위해 오디오 콘솔 및 네트워크 브릿지 등에 장착하는 네트워크 모듈로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Audinate Dante network module for network bridges and audio console expansion module

Compatible with network bridges and audio console expansion module

Enables multichannel recording and playback through Dante Virtual Soundcard (PC or Mac computer)

Primary and secondary Ethernet interfaces for dual-redundant Dante networking

Operates from internal Dante network Precision Time Protocol (PTP) clock or external clock via host unit

Optional Dante Controller software for remote configuration (PC or Mac computer)

LED indicators monitor network activity and speed

3. 규격 및 사양

Module format	: Cirrus CM-1 compatible

Sample rates	: 44.1/48/88.2/96 kHz

Audio channels (44.1/48kHz)	: Up to 64 bidirectional channels

Audio channels (88.2/96kHz)	: Up to 32 bidirectional channels

Sample Bit Depth	: 16, 24 or 32 bits per sample

Audio Buffering	: Up to 2000 samples per channel

Clock Source	: Onboard word clock or external word clock

Interfaces	: Primary and Secondary Dante network	interfaces

Dimensions (HxWxD)	: 31 x 110 x 89 mm

* KT-DANTE64 동급이상품