*) NETWORK MODULE

1. 개요

본 기기는 MADI 신호를 연결하기 위해 오디오 콘솔 및 네트워크 브릿지 등에 장착하는 네트워크 모듈로 다음과 같은 규격에 준한다.

2. 기능 및 특성

MADI (AES10-compliant) network module with up to 64 bidirectional channels @ 48 kHz and 32 bidirectional channels @ 96 kHz

Compatible with network bridges and audio console expansion module

Operates up to 500 m over optical fibre link and 200 m over coaxial copper link

Optical transmission on SC-Duplex connector

Copper transmission on 75 ohm coaxial BNC connectors

Dual-redundant operation with failover from optical to copper connections

Operates as either MADI clock master, MADI clock slave or from external clock via host unit

3. 규격 및 사양

Module format	: Cirrus CM-1 compatible

Sample rates	: 48 kHz, 96 kHz

Audio channels (48kHz)	: Up to 64 bidirectional channels

Audio channels (96kHz)	: Up to 32 bidirectional channels

Clock source	: MADI clock master, MADI clock slave or	external word clock

Optical fibre interface Transmit, Receive

- Connector type	: SC-Duplex

Coaxial copper interface Transmit, Receive

- Connector type	: 75 Ω BNC Dimensions

Dimensions (HxWxD)	: 31 x 110 x 89 mm

* KT-MADI 동급이상품