*) SPLITTER

1. 개요

본 기기는 오디오 신호를 증폭하여 분배하는 장비로 다음과 같은 규격에 준한다.

2. 기능 및 특성

12 channel microphone splitter with 2 electronically balanced and 2 transformer balanced outputs per channel

Solo bus with integrated headphone amplifier and level control

Independent +30 dB and -15 dB gain switches per channel

+48 V phantom power switch and earth lift switch per channel

Input and Output 1 duplicated on front and rear panels for cable looming fl exibility

Individual LED metering for each channel

Electronic outputs on rear panel for PA connections and front panel transformer outputs for broadcast feeds

Rugged 3U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Inputs

Input impedance	: > 2 kΩ

CMRR	: > -100 dB @ 100 Hz to 10 kHz

Equivalent input noise	: < -100 dBu @ unity gain

Signal present level	: > -25 dBu

Signal clip level	: > +21 dBu

Electronically-Balanced Outputs

Source impedance	: 50 Ω

Min load	: 600 Ω

Max level	: > +21 dBu @ 1 kHz

Connectors	: 3 pin male XLR (external),	3 way terminal strip (internal)

Frequency response	: +0 / -0.5 dB 20 Hz to 20 kHz

Distortion (THD+N)	: < 0.01% @ 1 kHz +4 dB

Transformer-balanced outputs

Source impedance	: 70 Ω

Min load	: 600 Ω (-3 dB level loss into 200 Ω )

Max level	: + 18 dBu @ 1 kHz

Connectors	: 3 pin male XLR (external),	3 way terminal strip (internal)

Frequency response	: +0 / -1.0 dB 20 Hz to 20 kHz

Distortion	: < 0.04% @ 1 kHz +4 dB

Audio Inputs / Outputs	: 3 pin XLR

Power	: IEC

Voltage	: 100 to 240V ± 10% 50/60 Hz <60W

Dimensions (WxDxH)	: 483 x 319 x 132 mm

Weight	: 7.4 kg

* DN1248PLS 동급이상품