*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

높은 전력 밀도 – 1U에서 2 x 100W

유연성 – Intelli Drive는 70V 또는 Low-Z(4, 8, 16옴)에서 채널당 등가의 전력을 제공함

비대칭 부하 – 임피던스가 다른 부하를 "믹싱 및 매칭"하여 전체 시스템 효율성과 자원의 활용을 모두 극대화 가능

자동 대기모드 기능 – 대기모드에서 소비전력 1와트 이하

고효율 – 매우 낮은 소비전력 및 효율적인 냉각회로의 발열 최소화

포괄적인 회로보호 및 오류정보 표시

3. 규격 및 사양

General

Number of channels	: 2

Total output all channels driven	: 200 W

Peak output voltage per channel	: 100 V / 70 Vrms

Max. output current	: 7.7 Arms

Max. Output Power (all ch.’s driven)

2 ohms	: N.R.

4 ohms	: 100 W

8 ohms	: 100 W

16 ohms	: 100 W (requires the “70 V” mode for the RSL,	“Lo-Z” gives 50 W)

70 V	: 100 W

100 V	: Can deliver 100 W to a 100 V load tapped at	200 W

Performance

THD 20 Hz - 20 kHz for 1 W	: <0.1%

THD at 1 kHz and 1 dB below clipping	: <0.05%

Signal To Noise Ratio	: >112 dBA

Channel separation (Crosstalk) at 1 kHz	: >70 dB

Frequency response	: 2 Hz - 40 kHz

Input impedance	: 20 kOhm

Common Mode Rejection (CMR)	: 50 dB

Output impedance	: 25 mOhm

Dimensions (WxHxD)	: 483 (19”) x 44 (1 U) x 276 mm

Weight	: 4.2 kg

Finish	: Dark grey aluminium front and black steel	chassis

* E2:2 동급이상품