*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

높은 전력 밀도 – 1U에서 4 x 500W

유연성 – Intelli Drive는 70V 또는 Low-Z(2, 4, 8옴)에서 채널당 등가의 전력을 제공함

비대칭 부하 – 임피던스가 다른 부하를 "믹싱 및 매칭"하여 전체 시스템 효율성과 자원의 활용을 모두 극대화 가능

자동 대기모드 기능 – 대기모드에서 소비전력 1와트 이하

고효율 – 매우 낮은 소비전력 및 효율적인 냉각회로의 발열 최소화

포괄적인 회로보호 및 오류정보 표시

3. 규격 및 사양

General

Number of channels	: 4

Total output all channels driven	: 2000 W

Max output voltage per channel	: 141 Vp / 100 Vrms

Max output current per channel	: 16.3 Arms

Sensitivity and Maximum Output Power (all ch. driven)

2 Ω load	: 1 dBu: 500 W @ 45 V mode

4 Ω load	: 4 dBu: 500 W @ 45 V mode

8 Ω load	: 3 dBu: 500 W @ 70 V mode

16 Ω load	: 3 dBu: 500 W @ 100 V mode

70 V load	: 4 dBu: 500 W @ 70V mode

100 V load	: 4 dBu: 500 W @ 100 V mode

Sensitivity and Maximum Output Power (single ch. max)

2 Ω load	: 1 dBu: 500 W @ 45 V mode

4 Ω load	: 3 dBu: 1000 W @ 70 V mode

8 Ω load	: 4 dBu: 1250 W @ 100 V mode

16 Ω load	: 4 dBu: 625 W @ 100 V mode

70 V load	: 4 dBu: 1100 W @ 70 V mode

100 V load	: 4 dBu: 1600 W @ 100 V mode

Performance

THD (20 Hz - 20 kHz @ 1 W into 8 Ω)	: <0.1%

THD @ 1 kHz, 1 dB below clipping	: <0.05%

Signal-to-noise ratio	: >106 dBA

Channel separation (crosstalk) @ 1 kHz	: >70 dB

Frequency response	: 2 Hz - 40 kHz

Input impedance	: 20 kΩ

Input common mode rejection, CMR	: 50 dB

Output impedance	: 25 mΩ

Dimensions (WxHxD)	: 483 (19”) x 44 (1 U) x 417 mm

Weight	: 7.9 kg

Finish	: Dark grey aluminium front and black steel	chassis

* E20:4 동급이상품