*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Four channels in one cabinet increases efficiency, flexibility and value in powering monitor systems, line arrays, and bi- or tri-amped systems. Adjacent channels bridgeable for 2- or 3-channel operation

Amplifiers maintain the impeccable sonic performance standards set by the original fP Series, with the same durability and even greater efficiency

Monitoring and control of key functions accessible via the intuitive DeviceControl software and the robust, daisy-chained NomadLink network, as well as by the leading third party control platforms

Road-proven output stage delivers Class B audio quality with Class D efficiency

Output power remains constant even with significant drops in the mains voltage

Unique, lightweight Intercooler® copper cooling system dissipates more heat to allow extended peak output

Selectable Gain, scalable Voltage Peak Limiter (VPL™), and bridge-mode operation allow custom configuration for any system or application

XLR input connectors

Heavy-duty binding post or speakON® output connectors

Excessive output current, DC, high temperature, very high frequency (VHF), short circuit, open load, mains fuse protection, and soft start

3. 규격 및 사양

General

Number of channels	: 4

Peak total output both channels driven	: 10000 W

Peak output voltage per channel	: 150 V

Max. output current per channel	: 50 A peak

Max. Output Power (Per ch. (both ch.’s driven) / Bridged per ch.)

2 ohms	: 2500 W / n.r.

4 ohms	: 2100 W / 5000 W

8 ohms	: 1300 W / 4200 W

16 ohms	: 660 W / 2600 W

Performance with Gain: 35 dB and VPL: 150 V

THD 20 Hz - 20 kHz for 1 W	: <0.1%

THD at 1 kHz and 1 dB below clipping	: <0.05%

Signal To Noise Ratio	: >112 dBA

Channel separation (Crosstalk) at 1 kHz	: >70 dB

Frequency response (1 W into 8 ohms) +0/-3 dB	: 6.8 Hz - 34 kHz

Input impedance	: 20 kOhm

Common Mode Rejection (CMR)	: >54 dB, 20 Hz to 20 kHz

Output impedance @ 100 Hz	: 32 mOhm

Dimensions (WxHxD)	: 483 (19”) x 88 (2 U) x 396 mm

Weight	: 12 kg

Finish	: Black painted steel chassis with black painted	steel / aluminum front

* FP10000Q 동급이상품