*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

스피커 프로세싱을 위한 강력한 DSP성능

검증된 D클래스의 안정적인 앰프 출력단

고효율의 스위치 모드 파워서플라이 (SMPS)

USB 연결을 통한 시스템 구성 및 모니터링 소프트웨어

간편한 설정 및 모니터링을 위한 직관적인 전면패널 사용자 인터페이스

쇼트 및 DC(직류), 과열 과부하에 대한 포괄적인 회로 보호

사용자 구성이 가능한 게인, 딜레이, 크로스오버, EQ, 리미터 및 다이내믹 EQ

최대 출력레벨과 드라이버의 안정적인 보호를 위한 스피커 보호 리미터

3. 규격 및 사양

General

Number of amplifier channels	: 2

Number of processing channels	: 2

Peak total output all channels driven	: 3000 W

Peak output voltage per channel	: 115 V

Peak output current per channel	: 32 A

Bridge mode	: No

Output circuit type	: Class-D

Amplifier Outputs

Max Output Power: All channels driven

- 2 Ω per channel	: 1000 W

- 4 Ω per channel	: 1500 W

- 8 Ω per channel	: 800 W

Audio Performance

THD+N 20 Hz - 20 kHz @ 1 W	: < 0.1%

THD+N @ 1kHz, 1 dB below clip	: < 0.1%

Signal-to-noise	: >90 dB

Channel separation (Crosstalk) @ 1 kHz	: >75 dB

Frequency response	: 10 Hz to 20 kHz, +0.5/ -1 dB

Input impedance	: 10 kΩ unbalanced, 20 kΩ balanced

Internal Sample rate	: 96 kHz

Product propagation delay	: 0.6 ms

Distortion,1/8 rated power	: < 0.1%

Dimensions (HxWxD)	: 93 x 483 x 326 mm

Weight	: 6.5 kg

Finish	: Black painted aluminium chassis and grey front

* PDX3000 동급이상품