*) DSP POWER AMP

1. 개요

본 기기는 DSP를 내장한 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

앰프 설계: TD®클래스 출력단

스위치모드 파워서플라이(R.SMPS™) 조정 장치는 전압의 급격한 변동 상황에서도 안정성 유지

광범위한 종류의 스피커 프리셋 데이터베이스(LoadLibrary™)

낮은 지연의 Dante 디지털 네트워크 기본 포함

선순위 및 후순위의 주/예비 네트워크 연결

0.1dB 단위로 조절 가능한 디지털 컨트롤 및 리콜 가능한 '증폭 게인'

-무한대에서 0dB까지 0.25dB 단계의 디지털 출력 어테뉴에이터(감쇄기)

샘플 구간에서 디지털 방식으로 구현된 제로 오버슈트 ISVPL(Inter-Sample Voltage Peak Limiting)은 17.8~194V(5K44의 경우 150V)에서 0.1V 단계로 조정 가능

전면 고해상도 LCD패널 디스플레이

모드 선택 및 메뉴 탐색을 위한 전면 방습 실리콘 처리된 터치패드 디스플레이 패널

Lake 고유의 클래식/선형위상/ FIR 스피커 프로세싱 및 Iso-Float™ 접지 절연이 있는 아날로그 입력

3. 규격 및 사양

General

Number of input channels	: 2

Number of output channels	: 4

Peak total output all channels driven	: 10800 W

Max. Peak output voltage per channel	: 153 V

Max. output current per channel	: 49 A peak

Max. Output Power (2 ohms / 4 ohms / 8 ohms / 16 ohms)

All channels driven	: 2350 W / 2300 W / 1300 W / 660 W

All channels driven into optimal impedance interval	: > 2700 W into 2.4 - 3.2 ohms

8 ohms bridged per ch.	: 4600 W

4 ohms bridged per ch.	: 4700 W

Bridged into optimal impedance interval	: >5400 W into 4.8 – 6.2 ohms

Audio Performance

THD + N 20 Hz - 20 kHz for 1 W : < 0.05%

THD + N at 1 kHz and 1 dB below clipping	: < 0.04%

Dynamic range with digital inputs (for all supported sample rates)	: > 116 dB

Dynamic range with analog inputs	: > 112 dB

Frequency response (1 W into 8 ohms, 20 Hz - 20 kHz)	: + /-0.05 dB

Common Mode Rejection (CMR)	: > 74 dB, 20 Hz to 20 kHz

Internal sample rate	: 96 k

Internal data path	: 32 bit floating point

Product propagation delay, best case (96 kHz AES)	: 1.61 ms

Product propagation delay, analog input	: 1.68 ms

Dimensions (WxHxD)	: 483 (19") x 88 (2 U) x 386 mm

Weight	: 13.5 kg

* PLM10000Q 동급이상품