*) ANALOGUE MIXER

1. 개요

본 기기는 아날로그 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Live performance and studio recording analogue mixer with 16 input channels

12 mono input channels with award-winning MIDAS microphone preamplifiers

2 electronically-balanced stereo line input channels on ¼ " TRS connectors

3 band EQ on mono channels with swept mid band

2 aux sends with pre/post fader switching

60 mm precision long-life faders

Rugged chassis construction for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Mono Inputs	: 12 x XLR, balanced

Line Input	: 1/4" TRS, balanced

Stereo Inputs	: 4 x 1/4 TRS connector, balanced

Equalizer
- Low	: ±15dB @ 80Hz, shelving
- Mid(mono inputs only)	: ±15dB @ 150Hz to 3.5kHz, variable semi-parametric
- High	: ±15dB @ 12kHz, shelving

Channel Inserts	: 1/4" TRS connector, unbalanced

Aux Sends	: 2 x 1/4" TRS connector, balanced

Monitor Out	: 2 x 1/4" TRS connector, balanced

Main Out	: 2 x XLR, electronically balanced

Main Out Inserts	: 2 x 1/4" TRS connector, unbalanced

Phones Output	: 1/4" TRS connector, unbalanced

2-Track Inputs	: 2 x RCA, unbalanced

Record Out	: 2 x RCA, unbalanced

Switch mode power supply	: 100~240V, 50/60Hz, switchable(T1.6A H250V)

Power consumption	: 40w

Dimensions	: W 438 x H 95 x D 370mm

Weight	: 5 kg

* DM16 동등이상품.