*) FIXED I/O BOX

1. 개요

본 기기는 Main Digital Mixer와 연동하여 사용가능한 Stage Box이다.

2. 규격 및 사양

Processing

A/D-D/A conversion	: 24-bit @ 44.1 / 48 kHz,	114 dB dynamic range (A-weighted)

Networked I/O latency	: 1.1 ms

Connectors

Programmable mic preamps, balanced XLR/TRS combo	: 8

Line outputs, balanced XLR	: 8

ULTRANET outputs, RJ45	: 2

AES50 port, SuperMAC networking, NEUTRIK etherCON	: 2

USB port for system updates, type B	: 1

Digital In/Out

AES50 SuperMAC networking @ 48 or 44.1 kHz, 24-bit PCM	: 2 x 48 Channels, bidirectional

AES50 SuperMAC cable length, CAT5 shielded	: < 80 m recommended

ULTRANET networking @ 48 or 44.1 kHz, 22-bit PCM	: 2

ULTRANET cable length, CAT5 shielded	: < 75 m

ULTRANET phantom power for P16-M personal mixers	: 2 powered outputs

Power

Switch-mode autorange power supply	: 100-240 V (50/60 Hz)

Power consumption	: 35 W

Powered over Ethernet (PoE)	: AES50-A PoE/SYNC IN

Physical

Dimensions	: 95 x 149 x 332 mm

Weight	: 2.45 kg

* DL8 동급이상품