*) FIXED I/O BOX

1. 개요

본 기기는 Main Digital Mixer와 연동하여 사용가능한 Stage Box이다.

2. 기능 및 특성

32 award-winning MIDAS PRO microphone preamplifiers with switchable 48 V phantom power

16 electronically balanced low impedance line level outputs

ULTRANET personal monitoring system connectivity for in-ear applications

Digital audio and control connectivity for TURBOSOUND speaker systems with ULTRANET networking capability

Dual AES50 SuperMAC ports for cascading additional DL16 stageboxes—no merger or router required

Automatic AES50 stage-split mode when connected between MIDAS M32 Series FOH and monitor consoles

Dual ADAT outputs providing 16-channel digital output on two optical TOSLINK* connectors

2 AES-3 ports (AES/EBU), for directly connecting PA system controllers with digital inputs

Remote operation via shielded CAT5e cable up to 330 ft / 100 m length

Mute All function for quietly patching any inputs on stage

MIDI In/Out for bidirectional communication between MIDAS M32 Series console and on-stage MIDI devices

Features Neutrik etherCON* AES50 and ULTRANET network ports

Rugged 3U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Processing

A/D-D/A conversion (Cirrus Logic A/D CS5368, D/A CS4398)	: 24-bit @ 44.1 / 48 kHz, 114 dB dynamic	range (A-weighted)

Networked I/O latency (stagebox in > console processing > stagebox out)	: 1.1 ms

Connectors

Programmable Midas mic preamps, balanced XLR	: 32

Line outputs, balanced XLR	: 16

AES/EBU outputs (AES3 XLR)	: 2

AES50 ports, SuperMAC networking, NEUTRIK etherCON	: 2

ULTRANET output, RJ45 (no power supplied)	: 1

MIDI inputs / outputs	: 1/1

ADAT outputs, Toslink	: 2

USB port for system updates, type B	: 1

Digital In/Out

AES50 SuperMAC networking @ 48 or 44.1 kHz, 24-bit PCM	: 2 x 48 channels, bidirectional

AES50 SuperMAC cable length, CAT5e shielded	: up to 100 m

ULTRANET networking @ 48 or 44.1 kHz, 22-bit PCM	: 1 x 16 channels, unidirectional

ULTRANET cable length, CAT5 shielded	: up to 75 m

ADAT output @ 48 or 44.1 kHz, 24-bit PCM	: 2 x 8 channels, unidirectional

Toslink optical, cable length	: 5 m, typical

AES/EBU output @ 48 or 44.1 kHz, 24-bit PCM	: 2 x 2 channels, unidirectional

XLR, 110 Ω balanced, cable length	: 5 m, typical

Power

Switch-mode autorange power supply	: 100-240 V (50/60 Hz)

Power consumption	: 55 W

Physical

Standard operating temperature	: 5°C to 40°C (41°F to 104°F)

Dimensions	: 483 x 242 x 138 mm

Weight	: 5.7 kg

* DL32 동급이상품.