*) DIGITAL AUDIO MIXING CONSOLE

1. 개요

본 기기는 디지털 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Live performance and studio recording digital console with up to 40 simultaneous input channels

16 award-winning Midas PRO microphone preamplifiers

25 time-aligned and phase-coherent mix buses

AES50 networking allows up to 96 inputs and 96 outputs

32 bi-directional channels of live recording/playback on dual SD/SDHC (cards not included)

Up to 3 hours of 32 channel PCM recording in one session - stored as uncompressed WAV files

High-performance aluminium and high-impact steel structure

Rack mount brackets included for ultimate flexibility

40 bit floating point digital signal processing

8 DCA and 6 mute groups

8 digital signal processing effects engines

17 Midas PRO motor faders

Daylight viewable 5" full colour TFT display screen

32 x 32 channel USB 2.0 audio interface

DAW remote control emulations of Mackie Control* and HUI* protocols

Optional wireless remote control with Midas Apps for iPhone* and iPad*

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Processing

Input Processing Channels	: 32 Input Channels, 8 Aux Channels, 8 FX	Return Channels

Output Processing Channels	: 8 / 16

16 aux buses, 6 matrices, main LRC	: 100

Internal Effects Engines (True Stereo / Mono)	: 8 / 16

Internal Show Automation (structured Cues / Snippets)	: 500 / 100

Internal Total Recall Scenes (incl. Preamplifiers and Faders)	: 100

Signal Processing	: 40-Bit Floating Point

A/D Conversion (8-channel, 96 kHz ready)	: 24-Bit, 114 dB Dynamic Range, A-weighted

D/A Conversion (stereo, 96 kHz ready)	: 24-Bit, 120 dB Dynamic Range, A-weighted

I/O Latency (Console Input to Output)	: 0.8 ms

Network Latency (Stage Box In > Console > Stage Box Out)	: 1.1 ms

Connectors

Midas PRO Series Microphone Preamplifier (XLR)	: 16

Talkback Microphone Input (XLR)	: 1

RCA Inputs / Outputs	: 2 / 2

XLR Outputs	: 8

Monitoring Outputs (XLR / ¼" TRS Balanced)	: 2 / 2

Aux Inputs/Outputs (¼" TRS Balanced)	: 6 / 6

Phones Output (¼" TRS)	: 1 (Stereo)

AES50 Ports (Klark Teknik SuperMAC)	: 2

Expansion Card Interface	: 32 Channel Audio Input / Output

ULTRANET P-16 Connector (No Power Supplied)	: 1

MIDI Inputs / Outputs	: 1 / 1

USB Type A (Audio and Data Import / Export)	: 1

USB Type B, rear panel, for remote control	: 1

Ethernet, RJ45, rear panel, for remote control	: 1

Display

Main Screen	: 5" TFT LCD, 800 x 480 Resolution, 262k	Colours

Channel LCD Screen	: 128 x 64 LCD with RGB Colour Backlight

Main Meter	: 18 Segment (-45 dB to Clip)

Power

Switch-Mode Power Supply	: Auto-Ranging 100-240 VAC (50/60 Hz) ± 10%

Power Consumption	: 70 W

Physical

Standard Operating Temperature Range	: 5°C – 40°C (41°F – 104°F)

Dimensions	: 478 x 617 x 208 mm

Weight	: 14.3 kg

* M32R LIVE 동급이상품.