*) ACTIVE MICROPHONE SPLITTER

1. 개요

본 기기는 24입력 24출력 오디오 신호 분배기로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 award-winning MIDAS microphone preamplifi ers per channel with switchable +48 V phantom power

2 dual redundant AES50 network ports with independent phase-locked loop synchronisation

24 electronically balanced output channels can be sourced from microphone preamplifiers or AES50 ports

Remote operation up to 100 m via CAT5/5e cable

24 bit audio operation with 96 kHz sample rate

All settings programmable from front panel controls or console

PSU status indicator LEDs and confi guration LCD display on front panel

Features Neutrik etherCON* AES50 network ports

Rugged 5U rackmount chassis for durability in portable applications

Dual redundant auto-ranging universal switch-mode power supplies

3. 규격 및 사양

XLR Connections

- 24 x (XLR) mic/line inputs (48 mic/line amps)

- 24 x (XLR) line outputs

Sampling frequency	: 48 kHz/96 kHz

Dynamic range @ 1 kHz	: 22 Hz to 22 kHz (at unity gain): > 107 dB

Maximum gain	: 45 dB

Crosstalk @ 1 kHZ	: -90 dB physically adjacent input channels

Crosstalk @ 10k HZ	: -90 dB physically adjacent input channels

Dimensions	: 5U x 410 mm deep

Net weight	: 15 kg

Power requirements	: 100 V to 240 V AC ±10%, 50 to 60 Hz

Power consumption	: <150 W

Operating temperature range	: +5° C to +40° C

Storage temperature range	: -20° C to +60° C

* DL231 동급이상품