*) PERSONAL MONITOR MIXER

1. 개요

본 기기는 48채널의 입력을 지원하는 퍼스널 모니터 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

MIDAS 모니터링 시스템 허브와 호환 가능한 듀얼 48채널 모니터 믹서

12개의 스테레오 그룹이 구성 가능한 스템 그룹으로 부터 믹스의 신속한 생성과 밸런싱을 가능하게 함

듀얼 믹스 기능으로 두 개의 완벽한 모니터 믹스에 대한 독립적인 제어 가능

리허설 세션과 공연의 스테레오 녹음 및 재생을 위한 통합 SD 카드 인터페이스

인-이어 모니터의 고립감을 없애기 위해 무대 사운드 피드를 제공하는 스테레오 엠비언스 마이크 내장

메인 콘솔과는 독립적으로 인-이어 믹스에 공간감을 더하는 스튜디오 품질의 리버브

POE(Power over Ethernet)를 지원하는 MIDAS 허브와 AES50 직접 연결을 통해 원격 전원 공급 가능

별도의 DC 전원을 공급할 경우, PoE 허브 없이 DP48을 데이지 체인 방식으로 연결 가능

Midas와 Behringer 디지털 콘솔 과 I/O 박스를 포함하여 AES50이 장착된 모든 44.1/48 kHz 장치와 호환 가능

AES50 입력 채널을 통해 Midas Pro 시리즈와 M32 콘솔의 입력 채널 레이블 및 색상 정보를 DP48 모니터 믹서와 공유 가능

무선 IEM 트랜스미터 연결을 위해 믹스를 콘솔/허브로 다시 보낼 수 있는 AES50 리턴 채널

차폐된 CAT5/5e 사용 시 100m까지 원격제어 가능 MIDAS 허브를 통한 DP48 모니터 믹서의 원격 셋업 및 제어

동일한 허브에 연결되었거나 데이지 체인으로 연결되었을 경우 다른 DP48에 대한 원격 제어 가능

고대비(High-contrast) 2.4” 컬러 TFT 디스플레이 화면에서 믹스 파라미터, 미터, 그룹 지정에 대한 명확한 개요 제공

로컬 클릭 트랙을 위한 아날로그 억스 입력

모든 스테이지 모니터링 환경에 적합한 고성능 헤드폰 출력

사운드 익스포져(Sound Exposure) 한도 안에서 안전한 모니터링 레벨이 가능하도록 완전하게 조절 가능한 리미터

DP48MB 어뎁터(별도 구매)를 이용하여 마이크 스탠드에 안전하게 장착 가능

3. 규격 및 사양

Connections

Phones Mix A / B	: 2 x 1/4" TRS, stereo, unbalanced, 25 Ω

Line Mix A / B	: 2 x 1/4" TRS, mono, balanced, 1 kΩ

: 2 x 1/4" TRS, mono, unbalanced, 500 Ω

Aux in	: 2 x 1/4" TRS, unbalanced, 20 kΩ

: 2 x 1/4" TRS, balanced, 40 kΩ

AES50 Thru / In	: 2 x RJ45

Equalizer

Low	: ±15 dB, semi-parametric, low shelving

Mid	: ±15 dB, semi-parametric, peak

High	: ±15 dB, semi-parametric, high shelving

Frequency	: 20 Hz to 22 kHz, adjustable

Output

Limiter	: Ratio ∞:1

Level, max.	: +12.8 dBu (Phones)

Mix A / Mix B	: 2 x stereo

AES50

Audio channels @ 48 kHz	: 48

Sample rate	: 44.1 / 48 kHz

Sample word length	: 24 bit

Clock synchronization	: AES50 IN

Latency	: min. 70 µs per node (AES50)

Cable	: Ethernet CAT 5e

Cable length	: max. 100 m

Data / Rec

SD/SDHC format	: FAT32

Card memory	: Up to 32 GB supported

Power Supply

AES50 input	: PoE (IEEE802.3af)

Power consumption	: max. 14 W (with DC adaptor)

Mains connection	: External power supply 24 VDC / 600 mA	(included)

Dimensions / Weight

Dimensions (H x W x D)	: 69 x 242 x 164 mm (2.72 x 9.53 x 6.46")

Weight	: 1.3 kg (2.9 lbs)

* DP48 동급이상품.