*) PERSONAL MIXER

1. 개요

본 기기는 퍼스널 믹서 또는 스테이지 박스와 호완이 가능한 4개의 POE 포트를 가진 모니터 시스템 허브로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Personal monitoring system hub with PoE remote powering for up to 4 DP48 personal mixers and compatible stage boxes

AES50 IN and THRU ports for cascading hubs or stage boxes with 48 bidirectional channels at 44.1/48 kHz

16 balanced analogue outputs for sending 4x2 personal stereo mixes to IEM transmitters in the side rack

Channel naming and Group assignments can be distributed from compatible M32 consoles

Midas DL8 Stage Boxes can be connected and powered from ports 1-4

Personal mix outputs can be monitored via AES50 upstream to connected consoles

Supports remote control forwarding of a DP48 personal mixer to another DP48

Front panel buttons for sending signals to analogue output groups 1-4, for StageConnect and for AES50-A upstream

StageConnect output with phantom power for connecting other StageConnect devices, providing 32-channel audio transmission at sub-millisecond latency,

24-Bit uncompressed PCM, 44.1/48 kHz, using balanced XLR cable (110-Ohm DMX recommended)

Remote operation via shielded CAT5e cable up up to 260 ft / 80 m recommended

Features Neutrik etherCON* AES50 network ports

Rugged 1U chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Connections

AES50 sync master / thru	: 2 x RJ45

AES50 remote outputs	: 4 x RJ45

Remote power	: PoE (IEEE802.3at)

USB	: Type B

StageConnect	: 1 x XLR, male

Analogue outputs	: 4 x XLR, balanced

: 12 x 1/4" TRS, balanced

Controls / Indicators

Power	: 1 x blue LED (button)

AES50-A	: 1 x green LED

: 1 x button LED, green/white

StageConnect	: 1 x green / white (button)

: 1 x green LED (port active)

Ports 1 - 4	: 4 x button LED, green/white

TO AES50-A	: 2 x green LED

AES50 - A / B	: 2 x green LED (good connection)

: 2 x red LED (error)

AES50

Audio channels	: 48

Sample rate	: 44.1 / 48 kHz

Sample word length	: 24 bit

Clock synchronization	: AES50 Sync Master

Latency	: min. 70 µs per node (AES50)

Cable	: shielded CAT 5e

Cable length	: up to 80 m (recommended)

StageConnect

Audio channels in / out	: 16 / 16

Sample rate	: 44.1 / 48 kHz

Sample word length	: 24 bit

Phantom power	: +12 V DC / 18 W

Latency	: < 0.1 ms

Cable	: XLR balanced, mic or DMX cable

Cable length	: max. 40 m (130 ft) with 110-Ohm DMX cable

Power Supply, Voltage, Current Consumption

Switch mode power supply	: Autorange, 100-240 V~50/60 Hz

Power consumption	: 180 W

Mains connection	: Standard IEC receptacle

Dimensions / Weight

Dimensions (H x W x D)	: 50 x 482 x 291 mm (1.97 x 18.98 x 11.46")

Weight	: 8.72 lbs / 3.96 kg

* HUB-4 동급이상품