*) HIGH-PERFORMANCE 2-WAY POINT-SOURCE ACTIVE SPEAKER

1. 개요

본 기기는 앰프내장형 2-WAY 포인트소스 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

134 dB Max SPL

Rotatable 100° x 70° TRW horn

12" neodymium woofer, 3.5" voice coil

3.0" Ti dome, neodymium compression driver

2 channel, 3200 W Class D Amplifier

DSP Processing with FiRPHASE and BMC

RDNet Networked Management

powerCON TRUE1 TOP mains connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 50 Hz ~ 20000 Hz

Max SPL @ 1m	: 134 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 70°

Transducers

Compression Driver	: 1.4" neo, 3.0" v.c

Woofer	: 12" neo, 3.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 750Hz

Protections	: Thermal, HF

Limiter	: Fast Limiter

Controls	: Gain Reduction, Proces., 8 sel. presets

RDNet	: Onboard

Power section

Total Power	: 3200 W Peak

High frequencies	: 1200 W Peak

Low frequencies	: 2000 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Quick lock, pole mount, 3 x M10 on top,	3 x M10 on bottom sides

Handles	: 2 on side

Pole mount/Cap	: 35 mm insert

Grille	: Steel with clothing

Color	: Black

Size

Height	: 620 mm / 24.41 inches

Width	: 360 mm / 14.17 inches

Depth	: 409.3 mm / 16.11 inches

* KX 32-A 동급이상품