*) HIGH-PERFORMANCE 2-WAY POINT-SOURCE ACTIVE SPEAKER

1. 개요

본 기기는 앰프내장형 2-WAY 포인트소스 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

127 dB max SPL

Rotatable 100° x 70° CMD horn

LF 2 x 5” neodymium woofer, 2” voice coil

HF 1.75” titanium dome, neodymium comp. driver

2 x Class-D amplifiers, 2000 Watts total power

DSP Processing with FiRPHASE and BMC

RDNet Networked Management

powerCON TRUE1 TOP mains connectors

Available in full black or white coating

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 70 Hz ~ 20000 Hz

Max SPL @ 1m	: 127 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 70°

Transducers

Compression Driver	: 1 x 1.0" neo, 1.75" v.c

Woofer	: 2 x 5.0" neo, 2.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 1200Hz

Protections	: Excurs.

Limiter	: Fast Limiter

Controls	: Bypass, Linear/High Pass, Volume

RDNet	: Onboard

Power section

Total Power	: 2000 W Peak

High frequencies	: 600 W Peak

Low frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 2X M10 TOP AND BOTTOM, 2X PIN D.10

Handles	: 2 TOP AND BOTTOM

Pole mount/Cap	: Quick-fit socket

Grille	: Steel with clothing

Color	: Black, White

Size

Height	: 456 mm / 17.95 inches

Width	: 154 mm / 6.06 inches

Depth	: 237.5 mm / 9.35 inches

Weight	: 9.8 kg / 21.61 lbs

* KX 515-A 동급이상품