*) ACTIVE TWO-WAY ARRAY SPEAKER

1. 개요

본 기기는 앰프내장형 2-WAY 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

135 dB max SPL

Rotatable 100° x 25° TRW waveguide

LF 2 x 10" neodymium woofer, 3.0" voice coil

HF 4.0" titanium dome, neodymium comp. driver

2 x Class-D amplifiers, 3200 Watt total power

DSP Processing with FiRPHASE and BMC

RDNet Networked Management

Advanced Rigging and powerCON TRUE1 TOP mains connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 45 Hz ~ 20000 Hz

Max SPL @ 1m	: 135 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 25°

Transducers

Compression Driver	: 1 x 1.4" neo, 4.0" v.c

Woofer	: 2 x 10" neo, 3.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: +4 dBu

Processor section

Crossover Frequencies	: 900Hz

Protections	: Thermal, RMS

Limiter	: Fast Limiter

Controls	: Gain Reduction, delay, proces., 8 sel. presets

RDNet	: Onboard

Power section

Total Power	: 3200 W Peak

High frequencies	: 1200 W Peak

Low frequencies	: 2000 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Array fittings, 2xM10 on the top, 2xM8

Handles	: 2 side, 2 rear

Pole mount/Cap	: 35 mm insert

Grille	: Steel with clothing

Color	: Black

Size

Height	: 825 mm / 32.48 inches

Width	: 310 mm / 12.2 inches

Depth	: 369 mm / 14.53 inches

Weight	: 30.4 kg / 67.02 lbs

* KXL 4-A 동급이상품