*) HIGH-PERFORMANCE ACTIVE SUBWOOFER

1. 개요

본 기기는 앰프내장형 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

129 dB max SPL

40 Hz to 400 Hz frequency range

2 x 8" neodymium woofers, 2.5" v.c.

2000 W Class-D Amplifier

RDNet Networked Management

Bass Motion Control excursion management

powerCON TRUE1 TOP mains connectors

Available in full black or white coating

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 400 Hz

Max SPL @ 1m	: 129 dB

Transducers

Woofer	: 2 x 8" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Protections	: Excurs.

Limiter	: Fast Limiter

Controls	: Volume

RDNet	: Onboard

Power section

Total Power	: 2000 W Peak

Low frequencies	: 2000 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 2X M20 TOP AND SIDE, 8X M10 2X SIDE

Handles	: 1 X SIDE

Pole mount/Cap	: 35 mm insert

Grille	: Steel with clothing

Color	: Black, White

Size

Height	: 243.5 mm / 9.59 inches

Width	: 603.5 mm / 23.76 inches

Depth	: 430 mm / 16.93 inches

Weight	: 20 kg / 44.09 lbs

* SUB 808-AS 동급이상품