*) ACTIVE TWO-WAY HIGH DEFINITION MONITOR

1. 개요

본 기기는 공연장, 종교 시설 등 다양한 환경에서 사용 할 수 있는 고출력 스테이지 모니터 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

131 dB SPL Max

1000W RMS, two-way Class-D amplifier

90° x 70° constant directivity coverage

Multifuncional cabinet with symmetrical transducers’ design

FiRPHASE

2 x 8" neodymium Woofers, 2.5" voice coil

Horn loaded 1.4" neo comp. driver, 3" voice coil

RDNet Networked Management

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 131 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 70°

Transducers

Compression Driver	: 1 x 1.5" neo, 3.0" v.c

Woofer	: 2 x 8" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 900 Hz

Protections	: Thermal, HF

Limiter	: Fast Limiter

Controls	: Bypass, Linear/High Pass, Volume, RDnet	on boar

RDNet	: Onboard

Power section

Total Power	: 2000 W Peak, 1000 W RMS

High frequencies	: 600 W Peak, 300 W RMS

Low frequencies	: 1400 W Peak, 700 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Handles	: 1 Top

Grille	: Steel

Color	: Black

Size

Height	: 318 mm / 12.52 inches

Width	: 445 mm / 17.52 inches

Depth	: 450 mm / 17.72 inches

Weight	: 14 kg / 30.86 lbs

* TT 20-CXA 동급이상품