*) ACTIVE THREE-WAY LINE ARRAY MODULE

1. 개요

본 기기는 앰프내장형 3-way 스피커로 라인 어레이 방식으로 설치하여 공연장, 경기장, 종교시설 등 중/대형 공간에 적합한 장거리 전송과 넓은 분산각도를 제공하는 제품으로 다음과 같은 규격에 준한다.

2. 기능 및 특성

8000 Watt power, 4 x onboard amplifiers

143 dB max SPL

RDNet networked management and monitoring

48 kHz, 32 bit DSP processing

2 x 12” neodymium woofers

4 x 6" neodymium woofer midrange

2 x 3” titanium dome neodymium compression drivers

Remarkably compact and lightweight

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 20000 Hz

Max SPL @ 1m	: 143 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 10°

Transducers

Compression Driver	: 2 x 1.4" neo, 3.0" v.c

Midrange	: 4 x 6.0" neo, 2.0" v.c

Woofer	: 2 x 12" neo, 3.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: +4 dBu

Processor section

Crossover Frequencies	: 200 Hz ~ 800 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Cluster size, HF correction, RDNET

RDNet	: Onboard

Power section

Total Power	: 8000 W Peak

High frequencies	: 2000 W Peak

Mid frequencies	: 2000 W Peak

Low frequencies	: 4000 W Peak

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Integrated Mechanics

Handles	: 2 side, 2 rear

Grille	: Steel

Color	: Black

Size

Height	: 366 mm / 14.41 inches

Width	: 1171 mm / 46.1 inches

Depth	: 502 mm / 19.76 inches

Weight	: 58.4 kg / 128.75 lbs

* HDL 50-A 4K 동급이상품