*) ACTIVE LINE ARRAY MODULE

1. 개요

본 기기는 앰프내장형 라인 어레이 스피커로 다양한 공간 및 용도에 적합한 장거리 전송과 넓은 분산각도를 제공하는 제품으로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1400 Watt Peak power - 700 Watt RMS

135 dB max SPL

55 Hz ~ 20 kHz frequency response

2 x 10" Woofers

1 x 3" Compression Driver

DSP controlled Input section with selectable presets

Tour grade safe and solid variable mechanics

Composite PP enclosure structurally wooden reinforced

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 55 Hz ~ 20000 Hz

Max SPL @ 1m	: 135 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 15°

Transducers

Compression Driver	: 1 x 2.0", 3.0" v.c

Woofer	: 2 x 10", 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 800 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Cluster, HF, High curving, Indoor

Power section

Total Power	: 1400 W Peak, 700 W RMS

High frequencies	: 400 W Peak, 200 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PP Composite

Hardware	: Rigging flyware

Handles	: 2 side, 2 back

Grille	: Steel

Color	: Black

Size

Height	: 294 mm / 11.57 inches

Width	: 705 mm / 27.76 inches

Depth	: 445 mm / 17.52 inches

Weight	: 30.2 kg / 66.58 lbs

* HDL 20-A 동급이상품