*) ACTIVE TWO WAY LINE ARRAY MODULE

1. 개요

본 기기는 앰프내장형 라인 어레이 스피커로 다양한 공간 및 용도에 적합한 장거리 전송과 넓은 분산각도를 제공하는 제품으로 다음과 같은 규격에 준한다.

2. 기능 및 특성

133 dB Max SPL

2000W Two-Way Amplifier

Exclusive FiRPHASE technology on-board

750 Hz Crossover for best vocal reproduction

RDNet Networked Management

3” Titanium Compression Driver

2 x 6” High-Powered Neodymium Woofers

4 PATH waveguide

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 55 Hz ~ 20000 Hz

Max SPL @ 1m	: 133 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 10°

Transducers

Compression Driver	: 1 x 1.5" neo, 3.0" v.c

Woofer	: 2 x 6.0" neo, 2.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: +4 dBu

Processor section

Crossover Frequencies	: 750 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Preset, RDNet bypass

RDNet	: Onboard

Power section

Total Power	: 2000 W Peak, 1000 W RMS

High frequencies	: 600 W Peak, 300 W RMS

Low frequencies	: 1400 W Peak, 700 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PP Composite

Hardware	: Array fittings

Handles	: 2 Back

Grille	: Steel

Color	: Black, White

Size

Height	: 237 mm / 9.33 inches

Width	: 470 mm / 18.5 inches

Depth	: 377 mm / 14.84 inches

Weight	: 13.5 kg / 29.76 lbs

* HDL 26-A 동급이상품