*) ACTIVE FLYABLE SUBWOOFER MODULE

1. 개요

본 기기는 라인 어레이 형태로 설치 가능한 앰프내장형 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

134 dB Max SPL

2200W Class-D Amplifier

40~140 Hz frequency response

RDNet Networked Management

1x15” Neodymium Woofer, 4.0” voice coil

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 140 Hz

Max SPL @ 1m	: 134 dB

Transducers

Woofer	: 1 x 15" neo, 4.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: +4 dBu

Processor section

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, Preset selection, RDnet on board

RDNet	: Onboard

Power section

Total Power	: 2200 W Peak, 1100 W RMS

Low frequencies	: 2200 W Peak, 1100 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Array fittings, 1 X M20

Handles	: 2 Side

Pole mount/Cap	: M20 thread

Grille	: Steel

Color	: Black, White

Size

Height	: 444 mm / 17.48 inches

Width	: 456 mm / 17.95 inches

Depth	: 508 mm / 20 inches

Weight	: 30 kg / 66.14 lbs

* HDL 35-AS 동급이상품