*) ACTIVE SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

2200 W

135 dB max SPL

35 Hz - 120 Hz frequency response

18" Woofer, 4.0" v.c.

Multi-ply hardwood polyurea-coated

Selectable gain, X-over, cardioid mode and time delay

Stereo XLR input, Stereo XLR signal output

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 35 Hz ~ 120 Hz

Max SPL @ 1m	: 135 dB

Transducers

Woofer	: 18", 4.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR

Output connectors	: XLR

Input sensitivity	: -2 dBu / +4 dBu

Processor section

Crossover Frequencies	: Selectable

Protections	: Thermal, RMS

Limiter	: dynamic limiter

Controls	: Gain, EQ, Xover, Delay, Cardioid

Power section

Total Power	: 2200 W Peak

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Handles	: One handle each side

Pole mount/Cap	: M20 thread

Grille	: Steel with clothing

Color	: Black

Physical specifications

Height	: 693 mm / 27.28 inches

Width	: 505 mm / 19.88 inches

Depth	: 685 mm / 26.97 inches

Weight	: 43.2 kg / 95.24 lbs

* SUB 8003-AS MK3 동급이상품