*) ACTIVE SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

1400 Watt Class-D Amplifier

18” Woofer, bass reflex housing

Stereo Crossover

Switchable Crossover Frequencies

Polarity-reverse switch

Electronic equalization, soft limiter and protection

Stereo XLR input, Stereo XLR signal output

Bass Motion Control excursion management

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 35 Hz ~ 120 Hz

Max SPL @ 1m	: 133 dB

Transducers

Woofer	: 1 x 18", 3.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Hi-Pass Frequencies	: 110Hz

Low-Pass Frequencies	: 80Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, EQ, Phase, Xover

Power section

Total Power	: 1400 W Peak, 700 W RMS

Low frequencies	: 1400 W Peak, 700 W RMS

Cooling	: Convection

Connections	: VDE

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Handles	: One each side

Pole mount/Cap	: M20 thread

Grille	: Steel with clothing

Color	: Black

Size / Weight

Height	: 693 mm / 27.28 inches

Width	: 505 mm / 19.88 inches

Depth	: 685 mm / 26.97 inches

Weight	: 40.6 kg / 89.51 lbs

* SUB 708-AS MK3 동급이상품