*) PROFESSIONAL ACTIVE STAGE MONITOR

1. 개요

본 기기는 공연장, 종교 시설 등 다양한 환경에서 사용 할 수 있는 스테이지 모니터 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 131 dB Sound Pressure Level

2100W Class-D bi-amplification

45-20000 Hz linear frequency response

1.75" Compression Driver

15" Woofer

FiRPHASE zero degrees phase technology

Bass Motion Control woofer excursion management

70ºx100º Constant Directivity Coverage Angle

Perfectly tailored for horizontal or vertical deployment

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 45 Hz ~ 20000 Hz

Max SPL @ 1m	: 131 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 70°

Transducers

Compression Driver	: 1 x 1.0", 1.75" v.c

Woofer	: 1 x 15", 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: Combo XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 1600 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Power section

Total Power	: 2100 W Peak

High frequencies	: 700 W Peak

Low frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Handles	: 1 on side and 1 on top

Pole mount/Cap	: 35 mm insert

Grille	: Steel

Color	: Black

Size / Weight

Height	: 357.3 mm / 14.07 inches

Width	: 705 mm / 27.76 inches

Depth	: 456.6 mm / 17.98 inches

Weight	: 23.8 kg / 52.47 lbs

* NX 915-SMA 동급이상품