*) PROFESSIONAL THREE-WAY ACTIVE SPEAKER

1. 개요

본 기기는 앰프내장형 3-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 138 dB Sound Pressure Level

2100W Class-D Amplifier

40-20000 Hz linear frequency response

1.75" Neodymium Compression Driver with Peek diaphragm

8" Midrange, 2.5" v.c.

15" High Power Woofer

Bass Motion Control and FiRPHASE processing

M10 Rigging Points

IP Rated Powercon TRUE1 TOP IN/OUT

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 20000 Hz

Max SPL @ 1m	: 138 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 60°

Transducers

Compression Driver	: 1 x 1.0'' neo, 1.75'' v.c

Midrange	: 1 x 8'' neo, 2.5'' v.c

Woofer	: 1 x 15", 3.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: Combo XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: Bass/Mid:320Hz, Mid/High:1200Hz

Protections	: Thermal, Excurs., RMS

Limiter	: Soft Limiter

Controls	: Linear, 2 Speakers, High Pass, Volume

Power section

Total Power	: 2100 W Peak

High frequencies	: 200 W Peak

Mid frequencies	: 500 W Peak

Low frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 3 x M10 Top, 1 x M10 each side,	1 x M10 bottom, 2 x M10 rear

Handles	: 1 x Side

Pole mount/Cap	: 35 mm insert

Grille	: Steel

Color	: Black

Size / Weight

Height	: 1075 mm / 42.32 inches

Width	: 461 mm / 18.15 inches

Depth	: 475 mm / 18.7 inches

Weight	: 45 kg / 99.21 lbs

* NX 985-A 동급이상품