*) ACTIVE COAXIAL STAGE MONITOR

1. 개요

본 기기는 공연장, 종교 시설 등 다양한 환경에서 사용 할 수 있는 스테이지 모니터 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

1400 Watt Peak, 700 Watt RMS digital bi-amplification

129 dB max spl

60° x 60° constant directivity horn

12" High power neodymium woofer, 2.5" voice coil

1.7" kapton dome, 1" exit, neodymium high frequency driver

DSP processing, floor - fre field equalization, soft limiter and protection

Combo XLR/JACK input, XLR signal output

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 50 Hz ~ 20000 Hz

Max SPL @ 1m	: 129 dB

Horizontal coverage angle	: 60°

Vertical coverage angle	: 60°

Transducers

Compression Driver	: Coaxial 1.0" neo, 1.75" v.c

Woofer	: 1 x 12" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: +4 dBu

Processor section

Protections	: RMS, HF

Limiter	: Soft Limiter

Controls	: Freefield, Floor

Power section

Total Power	: 1400 W Peak, 700 W RMS

High frequencies	: 400 W Peak, 200 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Handles	: 1 on side

Pole mount/Cap	: 35 mm insert

Grille	: Steel

Color	: Black

Size / Weight

Height	: 324 mm / 12.76 inches

Width	: 550 mm / 21.65 inches

Depth	: 417 mm / 16.42 inches

Weight	: 16.6 kg / 36.6 lbs

* NX 12-SMA 동급이상품