*) ACTIVE TWO-WAY ARRAY

1. 개요

본 기기는 스피커와 서브우퍼가 한 세트로 조합 된 앰프내장형 스피커로 우퍼 상단의 손잡이와 하단의 바퀴가 장착되어 이동이 용이하며, 빠르게 설치하여 사용 할 수 있는 제품으로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1400 Watt

130 dB max SPL

40 Hz ~ 20 kHz frequency response

15" Woofer

8 x 4" neodymium full-range woofer

90° x 30° slightly tilted pattern control

Innovative DSP processing

Pole mountable, easy set-up and transportation

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 20000 Hz

Max SPL @ 1m	: 130 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 30°

Transducers

Fullrange	: 8 x 4.0", 1.0" v.c

Woofer	: 15", 3.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 180 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, EQ

Power section

Total Power	: 1400 W Peak, 700 W RMS

High frequencies	: 400 W Peak, 200 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: VDE

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Color	: Black, White - RAL 9003

Size

Height	: 2200 mm / 86.61 inches

Width	: 410 mm / 16.14 inches

Depth	: 560 mm / 22.05 inches

Weight	: 36.4 kg / 80.25 lbs

* EVOX 12 동급이상품