*) ACTIVE TWO WAY ARRAY MUSIC SYSTEM

1. 개요

본 기기는 스피커와 서브우퍼가 한 세트로 조합 된 앰프내장형 스피커로 우퍼 상단의 손잡이와 하단의 바퀴가 장착되어 이동이 용이하며, 8채널 디지털 믹서가 장착되어 있는 제품으로 다음과 같은 규격에 준한다.

2. 기능 및 특성

128 dB Max SPL

1400 Watt 2-way power

8 IN Digital Mixer with multiple FX, Amp Simulator and Remote Control

DSP Processing with FiRPHASE

12" woofer, high power 2.5" voice coil

8 x 2" ultra compact fullrange 1.0" voice coil

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 40 Hz ~ 20000 Hz

Max SPL @ 1m	: 128 dB

Horizontal coverage angle	: 120°

Vertical coverage angle	: 30°

Transducers

Fullrange	: 8 x 2.0", 1.0" v.c

Woofer	: 1 x 12", 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 220 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, Boost, Mic/Line

Power section

Total Power	: 1400 W Peak, 700 W RMS

High frequencies	: 400 W Peak, 200 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: VDE

Electronic specifications

Frequency Response	: 20 Hz ~ 20 Hz

THD+N, 20dB gain, 0dBu out	: 0.004% A-Weighted

Processing

Processing Channels	: 8

Signal Processing	: 32 Bit Floating Point

A/D-D/A conversion	: 24 Bit @ 48.0 kHz

Dynamic Range	: 108

Inputs

Mic	: 4

Remote Controlled Storable Gain	: Yes

Gain Range	: 0 dB ~ 45 dB

Input Noise Level	: -114 dBu A-Weighted

Mic Inputs Impedance	: 3 kohm

Low Cut	: 20 Hz ~ 1000 Hz

Phantom Power +48V	: Yes

Mono Line	: 4

Gain Selection	: 0 dB ~ 45 dB

Line Input Impedance	: 11 kohm

HI-Z Line Inputs	: 1

HI-Z Line Inputs Impedance	: 1 Mohm

A/D Dynamic range	: 108 dB

Stereo Line	: 2

Gain Selection	: 0 dB ~ 45 dB

Stereo Line Input Impedence	: 11 kohm

Outputs

AUX Send	: 1

AUX Output	: 1

Outputs specifications

Main Out Impedance	: 150 ohm

Main Out Level	: 19 dBu

Aux Out Impedance	: 150 ohm

Aux Out Level	: 19 dBu

D/A Dynamic Range	: 108 dB

Compressors

Compressors	: 4 mono (6 preset)

EQ

Input Channels EQ	: 1 Semi Parametric / 2 Shelving

Description	: 3 Band EQ: High and Low band shelving,	Mid Band with sweepable frequency	: Graphic 7 Band EQ on Main Mix and AUX	send

Auxiliary sends

AUX	: 1 PRE/POST

FX POST	: 1

Internal Effects

Send Effects	: 1

MultiFX Insert Effects	: 1

Mastering processors

Main OUT processors	: 1

USB audio

Play trk	: 2

Other features

Footswitch	: Yes

Electrical specifications

Power supply	: Internal

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PP Composite

Handles	: 1 Top

Grille	: Steel

Color	: Black, White

Size

Height	: 623 mm / 24.53 inches

Width	: 400 mm / 15.75 inches

Depth	: 460 mm / 18.11 inches

Weight	: 22.2 kg / 48.94 lbs

* EVOX JMIX8 동급이상품