*) HIGH POWER TWO-WAY SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

800 W program power handling

129 dB max SPL

60 ~ 20000 Hz frequency range

90° x 70° constant directivity coverage angle

1 x 12" high power woofer

1 x 1.4" voice coil compression driver

High quality plywood cabinet

Installation points available on rear, top and bottom panels

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 129 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 70°

Directivity index Q	: 9

System Sensitivity	: 97 dB

Power section

Amplification	: Full Range

Nominal Impedance (ohm)	: 8 ohm

Power Handling	: 400 W

Peak Power Handling	: 1600 W PEAK

Protections	: Dynamic active mosfet

Crossover Frequencies	: 1800 Hz

Transducers

Compression Driver	: 1 x 1.0", 1.4" v.c

Woofer	: 1 x 12", 2.5" v.c

Input/Output section

Input connectors	: Speakon

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 2 x M8, 16 x M10

Pole mount/Cap	: 35 mm insert

Grille	: Steel with clothing

Color	: Black

Size

Height	: 620 mm / 24.41 inches

Width	: 362 mm / 14.25 inches

Depth	: 404 mm / 15.91 inches

Weight	: 22 kg / 48.5 lbs

* X MAX 12 동급이상품