*) TWO-WAY PASSIVE SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

300 W RMS power handling

126 dB max SPL

70 ÷ 20000 Hz frequency range

90° x 60° constant directivity coverage angle

1 x 8" high power woofer

1 x 1.5" voice coil compression driver

High quality Baltic birch plywood cabinet

Steel front grille with double mesh polyester clothing

Installation points available on rear, top and bottom panels

Speakon® NL4 connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 70 Hz ~ 20000 Hz

Max SPL @ 1m	: 126 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 60°

Directivity index Q	: 10

System Sensitivity	: 95 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 300 W

Peak Power Handling	: 1200 W PEAK

Protections	: Dynamic active mosfet

Crossover Frequencies	: 2000 Hz

Recommended Amplifiers	: QPS 10K, QPS 6.0K, IPS 5.0K, IPS 2.5K,	IPS 1.5K

Transducers

Compression Driver	: 1.0'', 1.5'' v.c

Woofer	: 8'', 2.0'' v.c

Input/Output section

Input connectors	: Speakon® NL4

Output connectors	: Speakon® NL4

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 6 x M8 (rear), 2 x M10 (lateral), multiplates	(top and bottom)

Pole mount/Cap	: M20 thread

Grille	: Steel with robust double mesh polyester	clothing

Color	: Black

Size

Height	: 427 mm / 16.81 inches

Width	: 242 mm / 9.53 inches

Depth	: 263 mm / 10.35 inches

Weight	: 12.2 kg / 26.9 lbs

* C 3108-96 동급이상품