*) TWO-WAY PASSIVE SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

600 W power handling (RMS)

137 dB max SPL

54 ÷ 20000 Hz frequency range

100° x 50° constant directivity coverage angle

1 x 12" high power neodymium woofer

1 x 3.0" v.c. neodymium compression driver

High quality birch plywood cabinet

Steel front grille with clothing

Installation points available on top, bottom, rear and side panels

SPEAKON in/out connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 54 Hz ~ 20000 Hz

Max SPL @ 1m	: 137 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 50°

Directivity index Q	: 10

System Sensitivity	: 97 dB

Power section

Amplification	: Full Range

Nominal Impedance (ohm)	: 8 ohm

Power Handling	: 600 W RMS

Peak Power Handling	: 2400 W PEAK

Protections	: Dynamic active mosfet

Crossover Frequencies	: 1100 Hz

Recommended Amplifiers	: XPS 16K, XPS 16KD, QPS 10K, QPS 6.0K,	IPS 5.0K, IPS 2.5K, IPS, 1.5K, DMA 504

Transducers

Compression Driver	: 1 x 1.4" neo, 3.0" v.c

Woofer	: 1 x 12'' neo, 3.5'' v.c

Input/Output section

Input connectors	: Speakon

Output connectors	: Speakon

Standard compliance

IP protection grade	: IP 21C

Safety agency	: CE compliant

EN54-24 certified	: Yes

CPR number	: 0068-CPR-234/2025

Physical specifications

Cabinet/Case Material	: Birch plywood

Hardware	: 4 x M8, 14 x M10

Grille	: Steel with clothing

Color	: Black - RAL 9005

Size

Height	: 620 mm / 24.41 inches

Width	: 361.8 mm / 14.24 inches

Depth	: 404 mm / 15.91 inches

Weight	: 23.5 kg / 51.81 lbs

* COMPACT C 32 동급이상품