*) TWO-WAY PASSIVE SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

60W AES power handling

113 dB max SPL

90 ~ 20000 Hz frequency range

120° x 120° constant directivity coverage angle

1 x 4" coax woofer

1 x 1" voice coil neodymium dome tweeter

High quality plywood cabinet

Wall mount bracket included

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 90 Hz ~ 20000 Hz

Max SPL @ 1m	: 113 dB

Horizontal coverage angle	: 120°

Vertical coverage angle	: 120°

Directivity index Q	: 6

System Sensitivity	: 89 dB

Power section

Nominal Impedance	: 16 ohm

Power Handling	: 60 W RMS

Peak Power Handling	: 240 W PEAK

Recommended Amplifier	: 120 W

Crossover Frequencies	: 1800 Hz

Transducers

Compression Driver	: 1.0" neo, 1.0" v.c

Nominal Impedance	: 16 ohm

Input Power Rating	: 10 W AES, 20 W PROGRAM POWER

Sensitivity	: 91 dB, 1W @ 1m

Woofer	: 4.0", 1.0" v.c

Nominal Impedance	: 16 ohm

Input Power Rating	: 60 W AES, 120 W PROGRAM POWER

Sensitivity	: 88 dB, 1W @ 1m

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 2 x M6, 2 x M8

Grille	: Steel with clothing

Color	: Black - RAL 9005, White - RAL 9003

Size

Height	: 148 mm / 5.83 inches

Width	: 132 mm / 5.2 inches

Depth	: 145 mm / 5.71 inches

Weight	: 2.3 kg / 5.07 lbs

* COMPACT M 04 동급이상품