*) TWO-WAY PROFESSIONAL SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

100 W RMS power handling

116 dB max SPL

60 ~ 20000 Hz frequency range

120° x 80° constant directivity coverage angle

1 x 6" high power woofer

1 x 1" voice coil neodymium dome tweeter

High quality plywood cabinet

Steel front grille with clothing

Installation points available on rear, top and bottom panels

4 pole EUROBLOCK connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 116 dB

Horizontal coverage angle	: 120°

Vertical coverage angle	: 80°

Directivity index Q	: 7

System Sensitivity	: 90 dB

Power section

Nominal Impedance	: 8 ohm

Power Handling	: 100 W RMS

Peak Power Handling	: 400 W PEAK

Recommended Amplifier	: 200 W

Protections	: Dynamic active mosfet

Crossover Frequencies	: 2200 Hz

Transducers

Compression Driver	: 1.3" neo, 1.0" v.c

Nominal Impedance	: 8 ohm

Input Power Rating	: 15 W AES, 30 W PROGRAM POWER

Sensitivity	: 92 dB, 1W @ 1m

Woofer	: 6.0", 1.5" v.c

Nominal Impedance	: 8 ohm

Input Power Rating	: 100 W AES, 200 W PROGRAM POWER

Sensitivity	: 90 dB, 1W @ 1m

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 4 x M6, 2 x M8

Grille	: Steel with clothing

Color	: Black - RAL 9005, White - RAL 9003

Size

Height	: 365 mm / 14.37 inches

Width	: 211 mm / 8.31 inches

Depth	: 232 mm / 9.13 inches

Weight	: 5.5 kg / 12.13 lbs

* COMPACT M 06 동급이상품